**ANNEXURE B**

**RFP 13/2015**

**TECHNICAL CRITERIA**

|  |  |
| --- | --- |
| **INDUSTRIAL FIXED SHREDDER EVALUATION CRITERIA** | |
| 1. **Characteristics**  * **Three-phase power** * **Terminal overload switch** * **Electronic control with reserve operation and automatic re-start** * **Conveyor device into the machine funnel** * **Conveyer belt into container (discharged shredding system)** * **Option of changing between Coarse, Medium and Fine Product Shaft Configuration** * **Should have a skip for disposing goods** | **35** |
| 1. **Dimensions**  * **Length - max 3.5m** * **Width - max 2300mm** * **Height - max 2500mm** * **Working Area (1350x1000mm)** | **20** |
| 1. **Performance**  * **Knife shafts with knives that can be individually changed and sharpened** * **Low noise and non-ballistic** * **Field of application should be, but not limited to CD's; computer hard drives and boards; carbon types; Tin and plastic cans; PET-bottles; Cigarettes; Wood, wooden boxes and pallets; Textiles ; Cable and electric waste or similar** | **15** |
| 1. **Warranty and maintenance**  * **Proof of warranty** * **Maintenance / Service plan to be provided with purchase of shredder(including spares)** * **Provision of training by an accredited service provider** | **15** |
| 1. **Reputation**  * **Submitted references from existing and previous clients, over the last five years** | **15** |
| **Total points** | **100** |